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ALAMO SEWER AND WATER GID 
Consumer Confidence Report – 2026 
Covering Calendar Year – 2025
[image: ]This brochure is a snapshot of the quality of the water that we provided last year. Included are the details about where your  water comes from, what it contains, and how it compares to Environmental Protection Agency (EPA) and state standards.  We are committed to providing you with information because informed customers are our best allies. It is important that  customers be aware of the efforts that are continually being made to improve their water systems. To learn more, please  attend any of the regularly scheduled meetings. 
For more information please contact at . 
Your water comes from:  

	SANDHILL WELL
	Ground Water



	 Industrial Park Well
	   Ground Water




We treat your water to remove several contaminants and we add disinfectant to protect you against microbial contaminants.  The Safe Drinking Water Act (SDWA) requires states to develop a Source Water Assessment (SWA) for each public water  supply that treats and distributes raw source water in order to identify potential contamination sources. The state has  completed an assessment of our source water. For results of the source water assessment, please contact us. 
Message from EPA 
Some people may be more vulnerable to contaminants in drinking water than the general population. Immuno-compromised  persons, such as those with cancer undergoing chemotherapy, persons who have undergone organ transplants, people with  HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These  people should seek advice about drinking water from their health care providers. EPA/CDC guidelines on appropriate means  to lessen the risk of infection by Cryptosporidium and other microbial contaminants are available from the Safe Drinking  Water Hotline (800-426-4791). 
Drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some  contaminants. The presence of contaminants does not necessarily indicate that water poses a health risk. More information  about contaminants and potential health effects can be obtained by calling the EPA’s Safe Drinking Water Hotline (800-426- 4791). 
The sources of drinking water (both tap water and bottled water) included rivers, lakes, streams, ponds, reservoirs, springs,  and wells. As water travels over the surface of the land or through the ground, it dissolves naturally occurring minerals and,  in some cases, radioactive material, and can pick up substances resulting from the presence of animals or from human  activity. 
Contaminants that may be present in source water before we treat it include: 
Microbial contaminants, such as viruses and bacteria, may come from sewage treatment plants, septic systems, agricultural  livestock operations and wildlife. 
Inorganic contaminants, such as salts and metals, can be naturally-occurring or result from urban storm water runoff,  industrial or domestic wastewater discharges, oil and gas production, mining or farming. 
Pesticides and herbicides may come from a variety of sources such as storm water run-off, agriculture, and residential users. Radioactive contaminants, can be naturally occurring or the result of mining activity 
Organic contaminants, including synthetic and volatile organic chemicals, which are by-products of industrial processes and  petroleum production, may also come from gas stations, urban storm water run-off, and septic systems. 
In order to ensure that tap water is safe to drink, EPA prescribes regulation which limits the amount of certain contaminants  in water provided by public water systems. We treat our water according to EPA’s regulations. Food and Drug  Administration regulations establish limits for contaminants in bottled water, which must provide the same protection for  public health. 
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Our water system tested a minimum of 1 sample(s) per month in accordance with the Total Coliform Rule for  microbiological contaminants. Coliform bacteria are usually harmless, but their presences in water can be an indication of  disease-causing bacteria. 

When coliform bacteria are found, special follow-up tests are done to determine if harmful bacteria  are present in the water supply. If this limit is exceeded, the water supplier must notify the public by newspaper, television  or radio. 
Water Quality Data 
The tables following below list all of the drinking water contaminants that were detected during the 2025 calendar year. The  presence of these contaminants does not necessarily indicate that the water poses a health risk. Unless noted, the data  presented in this table is from testing done January 1- December 31, 2025. The state requires us to monitor for certain  contaminants less than once per year because the concentrations of these contaminants are not expected to vary significantly  from year to year. Some of the data, though representative of the water quality, is more than one year old. The bottom line  is that the water that is provided to you is safe. 
[image: ]Terms & Abbreviations 
Maximum Contaminant Level Goal (MCLG): the “Goal” is the level of a contaminant in drinking water below which  there is no known or expected risk to human health. MCLG’s allow for a margin of safety. 
Maximum Contaminant Level (): the “Maximum Allowed” is the highest level of a contaminant that is allowed in  drinking water. ’s are set as close to the MCLG’s as feasible using the best available treatment technology. Action Level (): the concentration of a contaminant that, if exceeded, triggers treatment or other requirements that a water  system must follow. 
Treatment Technique (TT): a treatment technique is a required process intended to reduce the level of a contaminant in  drinking water. 
Maximum Residual Disinfectant Level (MRDL): the highest level of a disinfectant allowed in drinking water. There is  convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants. Maximum Residual Disinfectant Level Goal (MRDLG): the level of a drinking water disinfectant below which there is  no known or expected risk to health. MRDLG’s do not reflect the benefits of the use of disinfectants to control microbial  contaminants. 
Non-Detects (ND): laboratory analysis indicates that the constituent is not present. 
Parts per Million (ppm) or milligrams per liter (mg/l) 
Parts per Billion (ppb) or micrograms per liter (µg/l) 
Picocuries per Liter (pCi/L): picocuries per liter is a measure of the radioactivity in water. 
Millirems per Year (mrem/yr): measure of radiation absorbed by the body. 
Million Fibers per Liter (MFL): million fibers per liter is a measure of the presence of asbestos fibers that are longer than  10 micrometers. 
Nephelometric Turbidity Unit (NTU): nephelometric turbidity unit is a measure of the clarity of water. Turbidity in  excess of 5 NTU is just noticeable to the average person. 
[image: ]Testing Results for ALAMO SEWER AND WATER GID
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	Lead and Copper
	Date 
	90TH  
Percentile
	Range 
(low - high)
	Unit 
	AL 
	Sites  
Over  
AL
	Typical Source

	COPPER, FREE 
	2024
	.11
	0-.14
	ppm 
	1.3
	0 
	Corrosion of household plumbing systems;  Erosion of natural deposits; Leaching from  wood preservatives

	LEAD  
 
	2024 
	0
	0-1.2
	ppb 
	15
	0 
	Corrosion of household plumbing systems;  Erosion of natural deposits




	Regulated  
Contaminants
	Collection  
Date
	Highest  
Value
	Range 
	Unit 
	MCL 
	MCLG 
	Typical Source

	ARSENIC 
	11/24/25
	12
	0-12
	ppb
	10 
	0 
	Erosion of natural deposits; Runoff from  orchards; Runoff from glass and  
electronics production wastes 

	BARIUM 
	9/27/2021 
	0.11 
	0.11 
	ppm 
	2 
	2 
	Discharge of drilling wastes; Discharge  from metal refineries; Erosion of natural  deposits

	FLUORIDE 
	8/14/2024 
	1.1 
	0 - 1.1 
	ppm 
	2 
	4 
	Natural deposits; Water additive which  promotes strong teeth.

	NITRATE 
	8/14/2024 
	0.37 
	0 - 0.37 
	ppm 
	10 
	10 
	Runoff from fertilizer use; Leaching from  septic tanks, sewage; Erosion of natural  deposits




	Radionuclides 
	Collection  
Date
	Highest  
Value
	Range 
	Unit 
	MCL 
	MCLG 
	Typical Source

	COMBINED  
URANIUM
	7/29/25 
	28
	14 - 28 
	ug/L 
	30 
	0 
	Erosion of natural deposits





While your drinking water meets EPA's standard for arsenic, it does contain low levels of arsenic. EPA's standard balances the current understanding of arsenic's possible health effects against the costs of removing arsenic from drinking water. EPA continues to research the health effects of low levels of arsenic which is a mineral known to cause cancer in humans at high concentrations and is linked to other health effects such as skin damage and circulatory problems. Some people who drink water containing arsenic in excess of the MCL over many years could experience skin damage or problems with their circulatory system, and may have an increased risk of getting cancer.


Your water meets the EPA's standard for Lead. 
Lead can cause serious health effects in people of all ages, especially pregnant people, infants (both formula-fed and breastfed), and young children. Lead in drinking water is primarily from materials and parts used in service lines and in home plumbing. ALAMO SEWER AND WATER GID is responsible for providing high quality drinking water and removing lead pipes but cannot control the variety of materials used in the plumbing in your home. Because lead levels may vary over time, lead exposure is possible even when your tap sampling results do not detect lead at one point in time. You can help protect yourself and your family by identifying and removing lead materials within your home plumbing and taking steps to reduce your family's risk. Using a filter, certified by an American National Standards Institute accredited certifier to reduce lead, is effective in reducing lead exposures. Follow the instructions provided with the filter to ensure the filter is used properly. Use only cold water for drinking, cooking, and making baby formula. Boiling water does not remove lead from water. Before using tap water for drinking, cooking, or making baby formula, flush your pipes for several minutes. You can do this by running your tap, taking a shower, doing laundry or a load of dishes. If you have a lead service line or galvanized requiring replacement service line, you may need to flush your pipes for a longer period. If you are concerned about lead in your water and wish to have your water tested, contact ALAMO SEWER AND WATER GID at 702-556-8069. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at https://www.epa.gov/safewater/lead   Customer can recive a copy of the serivice line inventory by contacting the office at 253 Sanddhill road Alamo NV
2025 Violations
	Type 
	Category
	Analyte 
	Compliance Period

	MONITORING, ROUTINE MAJOR
	MON
	RADIUM -228
	1/1/2020-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	RADIUM-228
	1/1/2020-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	COMBINED RADIUM (-226&228)
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	ZINC
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	XYLENES, TOTAL
	1/1/2023/12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	VINYL CHLORIDE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	TRICHLOROETHYLENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	TRANS-1,2-DICHLOROETHYLENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	TOXAPHENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	TOTAL POLYCHLORINATED BIPHENYLS (PCB)
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJR
	MON
	TOLUENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJR
	MON
	THALLIUM, TOTAL
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJR
	MON
	TETRACHLOROETHYLENE
	1/1/2023-12/31/2025

	SATE FAILURE TO MONITOR
	MON
	TDS
	1/1/2023-12/31/2025

	SATE FAILURE TO MONITOR
	MON
	SULFATE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJR
	MON
	SODIUM
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJR
	MON
	SIMAZINE

	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	SILVER
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	SELENIUM
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	PICLORAM
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	PH
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
PENTACHLOROPHENOL
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	P-DICHLOROBENZENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	OXAMYL
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	ODOR
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
O-DICHLOROBENZENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
NITRITE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	NICKEL
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	METHOXYCHLOR 
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
MERCURY
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	
MBAS - FOAMING AGENTS (SURFACTANTS)
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	MANGANESE
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	MAGNESIUM
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	LASSO
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	
IRON
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	HEXACHLOROCYCLOPENTADIENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	HEXACHLOROBENZENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	HEPTACHLOR EPOXIDE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	HEPTACHLOR
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	GLYPHOSATE

	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR

	MON
	FLUORIDE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	ETHYLENE DIBROMIDE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	ETHYLBENZENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	ENDRIN
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	ENDOTHALL
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	DIQUAT
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	DINOSEB
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	DICHLOROMETHANE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
DI(2-ETHYLHEXYL) PHTHALATE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	DI(2-ETHYLHEXYL) ADIPATE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	DALAPON
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
CYANIDE
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	COPPER, FREE
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	
COLOR
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	CIS-1,2-DICHLOROETHYLENE

	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	CHROMIUM
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	CHLOROBENZENE
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	CHLORIDE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	CHLORDANE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	CARBON TETRACHLORIDE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	CARBOFURAN
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	CADMIUM
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
BHC-GAMMA
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	BERYLLIUM, TOTAL
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	BENZO(A)PYRENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	BENZENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	BARIUM
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
ATRAZINE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
ARSENIC
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	ANTIMONY, TOTAL
	1/1/2023-12/31/2025

	STATE FAILURE TO MONITOR
	MON
	ALUMINUM
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
2,4-D
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	2,4,5-TP 
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	1,2-DICHLOROPROPANE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	1,2-DICHLOROETHANE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	1,2-DIBROMO-3-CHLOROPROPANE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	1,2,4-TRICHLOROBENZENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	1,2,4-TRICHLOROBENZENE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	1,1,2-TRICHLOROETHANE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
1,1,1-TRICHLOROETHANE
	1/1/2023-12/31/2025

	MONITORING, ROUTINE MAJOR
	MON
	
REVISED TOTAL COLIFORM RULE (RTCR)
	1/1/2025-12/31/2025

	MONITORING, ROUTINE MAJOR
	
	NITRATE  
	1/1/2025-12/31/2025

	FOLLOW-UP OR ROUTINE TAP M/R (LCR)
	MON
	LEAD & COPPER RULE
	1/1/2025-12/31/2025

	STATE FAILURE TO MONITOR
	
	
IRON
	1/1/2025-12/31/2025

	MONITORING, ROUTINE MAJOR
	
	
FLUORIDE
	1/1/2025-12/31/2025

	MONITORING, ROUTINE MAJOR
	
	
COMBINED URANIUM
	1/12025-3/31/2025

	MONITORING, ROUTINE MAJOR
	
	
COMBINED URANIUM
	10/1/2025-12/31/2025 



· We are required to monitor your drinking water for specific contaminants on a regular basis. Results of regular monitoring are an indicator of whether or not our drinking water meets health standards. During [1/1/2025- 12/1/2025] we did not monitor or test’ or ‘did not complete all monitoring or testing’] for [arsenic, lead & copper, iocs, socs, ssocs, iron, fluoride, combined uranium, uranium, color, pH, TDS, sulfate nitrate] and therefore cannot be sure of the quality of your drinking water during that time
· Please share this information with all the other people who drink this water, especially those who may not have received this notice directly (for example, people in apartments, nursing homes, schools, and businesses). You can do this by posting this notice in a public place or distributing copies by hand or mail.

[image: ]There are no additional required health effects violation notices. 
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